4: SMS Mode Simulation

COMMANDS USED

1. **AT+CMGF=1**
   * Sets the modem to **Text Mode** for SMS messaging.
   * Returns OK if successful.
   * Without this, SMS would be in PDU (encoded) format, which is harder to read.
2. **AT+CMGS="9375984626"**
   * Prepares to send an SMS to the phone number 9375984626.
   * The emulator displays **“>”** indicating it is ready to accept the SMS text body.
   * After typing the message, pressing **Ctrl+Z** (^Z) tells the emulator to send it.
   * The emulator replied with:
     + +CMGS: 4 – a message reference number assigned to the sent this particular SMS.
     + OK – indicates that the message was successfully sent.
3. **AT+CMGR=1**
   * Tries to read the first stored SMS message.
   * The emulator responded with ERROR because message storage is not implemented in the CelerSMS AT Emulator.